
Update Steps for Mac:

1 . Please unplug the HDMI cable and power supply cable, only plug the JCA374 into the Type-C port on the Mac

2 . Upgrade tool and unzip this file.You will see two files (VL10XUpdateTool and JCA374-20170411.BIN)

3.Please click VL10XUpdateTool to execute the updating process and wait for the update to finish



Then unplug and replug in the JCA374 to verify the problem has been solved


-------------------------------------------------------------------------------------------------------------------------------------

MAC更新流程 :

1 . JCA374請先拔掉HDMI線與電源線 , 僅將JCA374插在Mac的TYPCE C Port上面

2 . 點選JCA347 FW upgrade tool檔案 , 在MAC上解壓縮之後您可以看到兩個檔案

VL10XUpdateTool跟JCA374-20170411.BIN

3 . 請點擊VL10XUpdateTool 

執行更新直到更新成功訊息出現 , 然後請拔除JCA374再插入確認使用即可